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DECLARATION OF COMPLIANCE


	Description
	Material
	Article Number

	Sous vide

	PE
	[bookmark: ArtNo]162016



Duni declares that the article meets the requirements of: 
· Article 3, 11(5), 15 and 17 of Regulation (EC) No 1935/2004 (Framework regulation) 
· EU Regulation 2023/2006/EC (GMP)
· EU Regulation 10/2011/EC with amendments (Plastic regulation)

Overall migration (1)
According to the above-mentioned regulation EU Regulation 10/2011, the overall migration does not exceed 10 mg/dm² or 60 mg/kg.

Specific migration (2)
This article contains monomers or additives subject to restrictions under the plastic regulation 10/2011 and its amendments. A specific migration test proves that these are within the limits. If more information regarding the monomers or additives are needed please contact Duni AB.
 
Area of use
Based on the migration tests and Declaration of Compliance in Duni’s possession, the articles can be used safely with all types of food under the following conditions: 
1. Any period at temperatures up to 40◦C
1. Periods up to 2 hours at temperatures up to 100◦C
1. Periods up to 1 hour at temperatures up to 121◦C

The bags are suitable for sous-vide cooking.



Test conditions
Migration tests on the article material performed by an independent institute showed that under the following test conditions, overall migration (see 1.) falls considerably below the limit given by regulation 10/2011.

Overall migration		
3% Acetic acid		10 days at 40°C, 1 hour at 121°C
	10 % Ethanol		10 days at 40°C, 1 hour at 121°C
	Vegetable oil		10 days at 40°C, 2 hours at 100°C

The ratio of food contact surface area to volume used is 6 dm²/kg

Dual Additives that might be present in the product:

	CAS No
	Substance

	471-34-1
	Carbonic acid, salts E170

	25322-68-3
	Polyethylene glycol E1521

	1309-48-4
	Magnesium oxide E530



The product does not contain any functional barrier.



Please be advised that Duni Group does not add anything into the product. 

This document of compliance is based on:
-	Documentation from suppliers
-	Global migration test
-	Specific migration 




This document was issued electronically and is therefore valid without signature.
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