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Product
Cooking bag
Raw Material
PE/PA/PE
Packaging
Inner: Polyethylene
Outer: Corrugated board 
Field Of Application
Cooking bag is typical used for cooking, storage and sterilization with aqueous, acidic and fatty food. The cooking bag may be used up to 40°C for 10 days, 100°C for 2 hours, and 121 °C for 1 hour.
EC Directive 94/62/EC on Packaging and Packaging Waste
The packaging complies with all essential requirements as defined by 94/62/EC. 
For example minimum adequate amount of packaging, limitation of heavy metal content, recyclable through at least one of the following: reuse, material recovery, energy recovery or composting.
Environmental Aspects
Product
Polyethylene is produced by refining of mineral oil or natural gas
Packaging
Polyethylene is made by refining of mineral oil or natural gas. 

The corrugated board box is to a large extend made of recycled fibers.






Product Safety
The products fulfil the following:
1. EU Regulation 1935/2004/EC, Material and products intended for contact with foodstuff.
1. EU Regulation 2023/2006/EC, Good Manufacturing Practice.
1. [bookmark: _GoBack]EU Regulation 10/2011/EC with amendments, Material and products of plastic produced for contact with foodstuff.
Migration tests on the article material performed by an independent institute showed that under appropriate test conditions, overall and specific (when relevant) migration falls considerably below the limit given by regulation 10/2011. For further details, see Declaration of Compliance.
1. Duni manufacturing units are certified according to the international quality system ISO 9001 and environmental system ISO 14001 as well as to BRC for hygiene. 
Management of Used Products
Energy Recovery
All the materials are suited for energy recovery. Complete combustion gives mainly rise to carbon dioxide and water. The energy content of plastics/paper is comparable to that of oil/ wood.
Recycling
Recycling of the plastic and the corrugated board is possible for producing new products. Check with the local recycling company.
Validity
This is a copy of a document issued 2018-02-19. It is normally updated every second year or when there is a change in the manufacturing process, in the product or in legislation. To make sure that you have the latest edition, contact Duni AB.
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