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DECLARATION OF COMPLIANCE

	Description
	Material
	Article Number

	Laminated bagasse bowls and trays 

	Bagasse fibre with PBAT/PLA
	[bookmark: ArtNo]205734



Duni declares that the article meets the requirements of: 
· Article 3, 11(5), 15 and 17 of Regulation (EC) No 1935/2004 (Framework regulation)
· EU Regulation 2023/2006/EC (GMP)
· EU Regulation 10/2011/EC with amendments
· BfR XXXVI (bagasse)
· Fluorinated substances in paper and cardboard food contact materials of the Ministry of Environment and Food of Denmark dated May 2018

Overall migration (1)
According to the above-mentioned regulations, the overall migration does not exceed 10 mg/dm² or 60 mg/kg.

Specific migration (2)
Duni's risk assessment of the product shows that the product contains no monomers or additives subject to restrictions under the plastic regulation 10/2011 and its amendments.

Area of use
Based on the migration tests and Declaration of Compliance, the article can be used for all kinds of foods under the following conditions:

· Long term storage in chilled conditions or room temperature
· Warm keeping at 70°C for up to 2 h or at 100°C for 15 minutes (hotfill[footnoteRef:1]) [1:  Definition from COMMISSION REGULATION (EU) 2016/1416: “hot-fill” means the filling of any article with a food with a temperature not exceeding 100 °C at the moment of filling, after which the food cools down to 50 °C or below within 60 minutes, or to 30 °C or below within 150 minutes.] 


The bowls are suitable to use in a microwave oven. However, it is the responsibility of the user of the finished packages to ensure that the package is safe to use in the intended conditions (W/min) taking into account all relevant information e.g. the shape and size of the package and packaged food.


Test conditions:
Migration tests on the article’s material performed by an independent institute showed that under the following test conditions overall migration (see 1.) and specific migration (see 2.; SML) fall considerably below the respective limits given by regulation 10/2011.

[bookmark: _Hlk153484309]Overall migration OM5[footnoteRef:2] [2:  OM5 test conditions corresponds to intended food contacts conditions “High temperature applications up to 121 °C” according to EU Regulation 10/2011/EC.] 

	Simulant
	Contact time
	Temperature
	Result (mg/dm3)

	10 % Ethanol
	2 hours
	100°C
	< 3

	3% Acetic acid
	2 hours
	100°C
	< 3

	95 % Ethanol
	4 hours
	60°C
	< 3

	Isooctane
	2 hours
	60°C
	< 3


	
Overall migration OM2[footnoteRef:3] [3:  OM2 standardised testing conditions corresponds to any long term storage at room temperature or below, including heating up to 70 °C for up to 2 hours, or heating up to 100 °C for up to 15 minutes as defined in Annex V, Chapter 3, table 3 in COMMISSION REGULATION (EU) No 10/2011 on plastic materials and articles intended to come into contact with food.] 

	Simulant
	Contact time
	Temperature
	Result (mg/dm3)

	10 % Ethanol
	10 days
	40°C
	< 3

	3% Acetic acid
	10 days
	40°C
	< 3

	95 % Ethanol
	10 days
	40°C
	< 3

	Isooctane
	2 days
	20°C
	< 3



Specific migration of PAA
	Simulant
	Contact time
	Temperature
	Result (mg/kg)

	3% Acetic acid
	2 hours
	100°C
	< 0,01



The ratio of surface area to volume is 5,4 dm²/kg.

No substances of dual use are present in the product.


Please be advised that Duni AB does not add anything into the product. 

This document of compliance is based on:
- Documentation from suppliers
- Global migration test


This document was issued electronically and is therefore valid without signature.
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