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DECLARATION OF COMPLIANCE

	Description
	Material
	Article Number

	Lids

	CPLA
	[bookmark: ArtNo]182536



Duni declares that the article meets the requirements of: 
· Article 3, 11(5), 15 and 17 of Regulation (EC) No 1935/2004 (Framework regulation) EU Regulation 2023/2006/EC (GMP)
· EU Regulation 2023/2006/EC (GMP)
· EU Regulation 10/2011/EC with amendments (Plastic regulation)

Overall migration (1)
According to the above mentioned regulations, the overall migration does not exceed 10 mg/dm² or 60 mg/kg.

Specific migration (2)
Duni's risk assessment of the product shows that the product contains no monomers or additives subject to restrictions under the plastic regulation 10/2011 and its amendments.
 
Area of use
The lids can be used safely with all types of beverages, serving cold and hot. The articles can be used for storage, hotfill[footnoteRef:1] and temperatures up to 2 hours at 70°C. [1:  Definition from COMMISSION REGULATION (EU) 2016/1416: “hot-fill” means the filling of any article with a food with a temperature not exceeding 100 °C at the moment of filling, after which the food cools down to 50 °C or below within 60 minutes, or to 30 °C or below within 150 minutes.] 


The lids are not suitable to use in microwave oven.


Test conditions
Migration tests on the material of the article performed by an independent institute showed that under the following test conditions overall migration (see 1.) and specific migration (see 2.) fall below the respective limits given by regulation 10/2011.

Overall migration				3% Acetic acid	2 hours at 70°C
							20 % Ethanol	2 hours at 70°C
95 % Ethanol	2 hours at 60°C
Isooctane		0,5 hours at 40°C

Specific migration on metals			3% Acetic acid	2 hours at 70°C

	

The ratio of food contact surface area to volume used is 6 dm²/kg

No substances of dual use are present in the product.

The product does not contain any functional barrier.


Please be advised that Duni AB does not add anything into the product. 

This document of compliance is based on:
-	Documentation from suppliers
-	Global migration test
-	Specific migration 



This document was issued electronically and is therefore valid without signature.
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